massRange {rawrr} | R Documentation

## Acquisition/scan range of spectrum

### Description

Acquisition/scan range of spectrum

### Usage

    massRange(x)

### Arguments

`x` | A rawrrSpectrum object

### Value

A double vector of length two. The first component is the start m/z, the second is the stop m/z value used by the detector during data acquisition. Also referred to as scan range.

### Examples

    S <- readSpectrum(rawfile = sampleFilePath(), 1)
    massRange(S[[1]])

[Package rawrr version 1.2.0 Index]