chipAddressToSignal {sesame} | R Documentation

## Lookup address in one sample

### Description

Lookup address and transform address to probe

### Usage

    chipAddressToSignal(dm, mft)

### Arguments

`dm` | data frame in chip address, 2 columns: cy3/Grn and cy5/Red
`mft` | a data frame with columns Probe_ID, M, U and col

### Details

Translate data in chip address to probe address. Type I probes can be separated into Red and Grn channels. The methylated allele and unmethylated allele are at different addresses. For type II probes methylation allele and unmethylated allele are at the same address. Grn channel is for methylated allele and Red channel is for unmethylated allele. The out-of-band signals are type I probes measured using the other channel.

### Value

a SigDF, indexed by probe ID address

[Package sesame version 1.12.9 Index]