flow_iQC {flowAI} | R Documentation

## Interactive quality control of Flow Cytometry Data

### Description

The call of the `flow_iQC` function opens a Shiny application that allows to perfom a complete and interactive quality control of an FCS file. The framework of the interactive quality control is complementary to the automatic one of the `flow_auto_qc` function. Hence, the anomalies are manually selected from the evaluation of three main properties of flow cytometry: 1) flow rate, 2) signal acquisition, 3) dynamic range.

### Usage

    flow_iQC()

### Author(s)

Chen Hao, Gianni Monaco

### Examples

    if (interactive()) flowAI::flow_iQC()

[Package flowAI version 1.6.3 Index]