Working Implementation

Agreements for Open Systems

Interconnection Protocols:

Part 14 - Virtual Terminal

Output from the September 1993 Open Systems

Environment Implementors’ Workshop (OIW)

SIG Chair: Michelle Conaway, HFSI

SIG Editor: Scott Wattum, Digital Equipment Corp., Workshop Editor: Brenda

Gray

Foreword

This part of the Working Implementation Agreements was prepared by the Virtual Terminal Special Interest

Group (VTSIG) of the Open Systems Environment Implementors’ Workshop (OIW). See Procedures

Manual for Workshop charter.

Text in this part has been approved by the Plenary of the above-mentioned Workshop. This part replaces

the previously existing chapter on this subject.

Only the pages that were changed in December 1992 are being printed. Please refer to the September

1992 Working Document for additional information.

Three normative annexes are given.

Future changes and additions to this version of these Implementor Agreements will be published as a new

part. Deleted and replaced text will be shown as strikeouts. New and replacement text will be shown as

shaded.

Table of Contents

Part 14 ISO Virtual Terminal Protocol . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1

0 Introduction . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1

1 Scope . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1

1.1 Phase Ia agreements . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1

1.2 Phase Ib agreements . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1

1.3 Phase II agreements . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1

2 Normative references . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1

3 Status . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2

3.1 Status of phase Ia . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2

3.2 Status of phase Ib . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2

3.3 Status of phase II . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2

4 Errata . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2

5 Conformance . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 3

6 Protocol . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 3

7 OIW registered control objects . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 3

7.1 Sequenced Application (SA) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 3

7.2 Unsequenced Application (UA) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 3

7.3 Sequenced Terminal (ST) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 3

7.4 Unsequenced Terminal (UT) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 3

7.5 Termination Conditions CO (TC) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 4

7.5.1 Entry number . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 4

7.5.2 Name of sponsoring body . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 4

7.5.3 Date . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 4

7.5.4 Identifier . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 4

7.5.5 Descriptor value . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 4

7.5.6 CO VTE-parameters . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 4

7.5.7 CO values, semantic and update syntax . . . . . . . . . . . . . . . . . . . . . . . . 5

7.5.8 Additional information . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6

7.5.9 Usage . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6

8 OIW defined VTE-profiles . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6

8.1 Telnet profile . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6

8.2 Transparent profile . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6

8.3 Forms profile . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6

8.4 X3 profile . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6

8.5 Generalized Telnet profile . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6

8.6 Scroll profile . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 7

8.6.1 Introduction . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 7

8.6.2 Association requirements . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 7

8.6.2.1 Functional units . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 7

8.6.2.2 Mode . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 7

8.6.3 Profile body . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 7

8.6.4 Profile argument definitions . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 12

8.6.5 Profile dependent CO information . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 13

8.6.6 Profile notes . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 13

8.6.6.1 Definitive notes . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 13

8.6.6.2 Informative notes . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 13

8.6.7 Specific conformance requirements . . . . . . . . . . . . . . . . . . . . . . . . . . . 15

8.7 S-mode Paged Application profile . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 15

Annex A (normative)

Specific ASE requirements . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 16

Annex B (normative)

Clarifications . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 17

Annex C (normative)

Object identifiers . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 18

Annex E — ( — normative

— )—

OIW X — —

OSI— contributions

— . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 26 —

E— .1— XDMCP— —

OSI—

. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 26 —

E— .1.1

— Introduction— . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 26 —

E— .1.2

— Functional— — overview— . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 26 —

E— .1.2.1

— ACSE— — requirements— . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 26 —

E— .1.2.2

— Presentation— — requirements— . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 26 —

E— .1.2.3

— Session— — requirements— . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 27 —

E— .1.2.4

— Abstract— — and— — transfer— — syntaxes— . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 27 —

E— .1.2.5

— XDMCP— — to— — OSI— — mapping— . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 27 —

E— .1.2.5.1

— Query— -— display— — to— manager— . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 27 —

E— .1.2.5.2

— IndirectQuery— -— display— — to— — manager— . . . . . . . . . . . . . . . . . . . . . . . . . . . 28 —

E— .1.2.5.3

— IndirectQuery— -— manager— — to— manager— . . . . . . . . . . . . . . . . . . . . . . . . . . 28 —

E— .1.2.5.4

— Indirect— — query— -— manager— — to— display— . . . . . . . . . . . . . . . . . . . . . . . . . . . 29 —

Part 14 ISO Virtual Terminal Protocol

Editor’s Note - References to Stable Agreements in this part refer to Version 5.

0 Introduction

See Stable Agreements.

1 Scope

1.1 Phase Ia agreements

See Stable Agreements.

1.2 Phase Ib agreements

See Stable Agreements regarding Forms profile.

The Scroll profile is intended to support line-at-a-time applications and has colour and text attribute

capabilities.

1.3 Phase II agreements

See Stable Agreements regarding X.3 profile, Generalized Telnet profile and the S-mode Paged

Application Profile.

2 Normative references

See Stable Agreements.

3 Status

These agreements are being done in phases. Below is the current status of each phase.

3.1 Status of phase Ia

The Phase Ia Agreements, which include the profiles for Telnet and Transparent operation, are complete

and were stabilized in May, 1988. See Stable Agreements.

3.2 Status of phase Ib

The Forms profile of Phase 1b was stabilized in December, 1988. Alignment with EWOS Forms profile

was achieved in September, 1989. See Stable Agreements.

3.3 Status of phase II

Phase II is still in progress and includes the remaining profile work for the Scroll profile.

The S-mode Paged Application Profile is being progressed as PDISP 11187-2 (AVT-23 S-mode Paged

Application Profile).

The X.3 profile was stabilized in December 15, 1989.

The Generalized Telnet profile was stabilized in December 13, 1991.

It is intended that Phase II agreements be compatible with Phase I agreements.

4 Errata

See Stable Agreements.

5 Conformance

See Stable Agreements.

6 Protocol

See Stable Agreements.

7 OIW registered control objects

7.1 Sequenced Application (SA)

See Stable Agreements.

7.2 Unsequenced Application (UA)

See Stable Agreements.

7.3 Sequenced Terminal (ST)

See Stable Agreements.

7.4 Unsequenced Terminal (UT)

See Stable Agreements.

7.5 Termination Conditions CO (TC)

This CO is an instance of the standard type TCCO, as defined in ISO 9040. It is initially designed for use

with the OIW Scroll VT profile, though as a registered CO it is available for use by other VT profiles.

In addition to the three standardized data elements, it provides a definition and update syntax for further

types of Termination Condition. Each additional type is available for use in additional data elements of the

CO. The number and type of such additional data elements is defined in the profile using this CO.

7.5.1 Entry number

To be supplied by the Registration Authority.

7.5.2 Name of sponsoring body

OSI Implementors’ Workshop for Implementors of OSI, VTSIG.

7.5.3 Date

The date of submission of this proposal is September 15, 1989.

7.5.4 Identifier

oiw-vt-co-tcco-tc OBJECT IDENTIFIER ::= { oiw-vt-co-tcco tc(0) }

7.5.5 Descriptor value

"OIW VT CO for Termination Conditions"

7.5.6 CO VTE-parameters

CO-structure = , *(not defined in this registration, see note 1 in 14.7.5.8)*

CO-priority = "normal"

{

CO-element-id = 1, *(termination length)*

CO-category = "integer",

CO-size = 65535 },

{

CO-element-id = 2, *(time-out mantissa)*

CO-category = "integer",

CO-size = 65535 },

{

CO-element-id = 3, *(time-out exponent)*

CO-category = "integer",

CO-size = 65535 },

*(the following represents possibly multiple invocations of a generic data element type, according to the

value of CO-structure for the instance of this CO. )*

FOR N=4 to CO-structure

{

CO-element-id = N, *(acts as integer identifier for the events in this element)*

CO-category = "transparent",

CO-size = *(not defined in this registration, see note 2 in 14.7.5.8)* }

7.5.7 CO values, semantic and update syntax

The value fields for data elements 1,2 and 3 are defined in ISO 9040.

The value field for each additional data element is defined by the following ASN.1 construct which also

defines the update syntax.

TermCondList ::= SEQUENCE OF CHOICE {

void [0] IMPLICIT NULL,

x3ForwardingCond [1] IMPLICIT INTEGER,

stEventList [2] IMPLICIT Range,

anySTUpdate [3] IMPLICIT NULL,

stEventMasks [4] IMPLICIT MaskValues,

dOChars [5] IMPLICIT DOCharacters }

Range ::= SEQUENCE OF SEQUENCE {

[1] IMPLICIT LogEvent,

[2] IMPLICIT LogEvent OPTIONAL }

-- each pair represents an interval of values as defined for the value field of

--CO ST, see 14.7.3.7. The second value in each pair shall not be smaller than

--the first value. If the second value is omitted, the interval contains only

--the specified first value.

LogEvent ::= INTEGER

-- values as defined for value field of CO ST, see 14.7.3.7.

MaskValues ::= SEQUENCE OF SEQUENCE {

mask [1] IMPLICIT LogEvent,

value [2] IMPLICIT LogEvent }

DOCharacters ::= SEQUENCE OF SEQUENCE {

[1] IMPLICIT Repref,

[2] IMPLICIT INTEGER,

[3] IMPLICIT INTEGER OPTIONAL }

Repref ::= INTEGER

-- index to the list of repertoires for the Display Object

7.5.8 Additional information

NOTE - The value of CO-structure is defined in the profile to be the number of types of termination conditions

available for use within the profile.

NOTE - The value of CO-size for each additional data element of this CO must be defined within the profile

definition which uses those additional termination conditions.

7.5.9 Usage

Defined in profile.

8 OIW defined VTE-profiles

8.1 Telnet profile

See Stable Agreements.

8.2 Transparent profile

See Stable Agreements.

8.3 Forms profile

See Stable Agreements.

8.4 X3 profile

See Stable Agreements.

8.5 Generalized Telnet profile

See Stable Agreements

8.6 Scroll profile

OIW VTE-Profile Scroll-1989 (r1,r2,...r9)

8.6.1 Introduction

This Scrolling A-mode VTE-profile is designed to support line-at-a-time interactions between a terminal and

a host system, the type of operation typified by operating system command entry.

Scrolling is bi-directional, forward and backward.

The profile also provides a facility for switching local echo "on" or "off".

This VTE-Profile supports what is often referred to as "type-ahead", so input from the terminal user is

available to the host application as soon as the application is ready for input, thus providing efficiency by

minimizing communication delays.

This VTE-profile supports the definition of "input" termination events by the "Application VT-user" so the

application can specify what events will cause "input" data to be forwarded to the "Application VT-user".

8.6.2 Association requirements

8.6.2.1 Functional units

The Urgent Data Functional Unit is optional, and will be used if available.

8.6.2.2 Mode

This profile operates in A-mode.

8.6.3 Profile body

Display-objects =

{

{

display-object-name = DOA,

DO-access = profile-argument-rl,

dimension = "two",

x-dimension =

{

x-bound = profile-argument-r2,

x-addressing = "no-constraint",

x-absolute = "no", x-window = x-bound

},

y-dimension =

{

y-bound = "unbounded",

y-addressing = "no-constraint",

y-absolute = "no",

y-window = profile-argument-r10

},

erasure-capability = "yes",

*( repertoire-capability is implied by the number of occurrences of profile-argument-r4 )*

repertoire-assignment = profile-argument-r4,

DO-emphasis = profile-argument-r5,

foreground-colour-capability = profile-argument-r6,

foreground-colour-assignment = profile-argument-r7,

background-colour-capability = profile-argument-r6,

background-colour-assignment = profile-argument-r8

},

{

display-object-name = DOB,

DO-access = opposite of profile-argument-rl,

dimension = "two",

x-dimension =

{

x-bound = profile-argument-r2,

x-addressing = "no-constraint",

x-absolute = "no",

x-window = x-bound

},

y-dimension =

{

y-bound = "unbounded",

y-addressing = "higher only",

y-absolute = "no",

y-window = 1

},

erasure capability = "yes",

*( repertoire-capability is implied by the number of occurrences of profile-argument-r4 )*

repertoire-assignment = profile-argument-r4,

DO-emphasis = profile-argument-r5,

foreground-colour-capability = profile-argument-r6, foreground-colour-assignment = profile-argument-r7,

background-colour-capability = profile-argument-r6,

background-colour-assignment = profile-argument-r8

}

},

Control-objects =

{

{

CO-name = E, *(standard Echo CO)*

CO-type-identifier = vt-b-sco-echo,

CO-access = profile-argument-r1,

CO-priority = "normal",

CO-trigger = "selected",

CO-category = "boolean",

CO-size = 1

},

IF r9 = "TE" THEN

{

CO-name = TE, *(Termination Event CO)*

CO-type-identifier = vt-b-sco-tco,

CO-access = opposite of profile-argument-r1,

CO-priority = "normal",

CO-trigger = "selected",

CO-category = "integer"

},

{

CO-name = SA, *(NIST Registered CO)*

CO-type-identifier = nist-vt-co-misc-sa,

CO-access = profile-argument-r1,

CO-priority = "normal",

CO-trigger = "not selected",

CO-category = "integer",

CO-size = 65535

},

{

CO-name = UA, *(NIST Registered CO)*

CO-type-identifier = nist-vt-co-misc-ua,

CO-access = profile-argument-r1,

CO-priority = "urgent",

CO-category = "integer",

CO-size = 65535

},

{

CO-name = ST, *(NIST Registered CO)*

CO-type-identifier = nist-vt-co-misc-st,

CO-access = opposite of profile-argument-r1,

CO-priority = "normal",

CO-category = "integer",

CO-size = 65535

},

{

CO-name = UT, *(NIST Registered CO)*

CO-type-identifier = nist-vt-co-misc-ut,

CO-access = opposite of profile-argument-r1,

CO-priority = "urgent",

CO-category = "integer",

CO-size = 65535

},

{

CO-name = TC, *(Termination conditions CO)*

CO-type-identifier = nist-vt-co-tcco-tc,

CO-structure = N, *( defined with TCCO)*

CO-access = profile-argument-r1,

CO-priority = "normal",

{

CO-element-id = 1, *(termination length)*

CO-category = "integer",

CO-size = 65535 },

{

CO-element-id = 2, *(time-out mantissa)*

CO-category = "integer",

CO-size = 65535 },

{

CO-element-id = 3, *(time-out exponent)*

CO-category = "integer",

CO-size = 65535 },

{

CO-element-id = 4-N, *(from registered TCCO)*

CO-category = ???,

CO-size = ??? }

The NIST Workshop VT SIG is defining this registered TCCO. This

TCCO is a reference to that registered control object.

}

}

Device-objects =

{

{

device-name = DVA, *("output" device object)*

device-default-CO-access = profile-argument-rl,

device-default-CO-initial-value = 1."true",

device-display-object = DOA,

device-minimum-X-array-length = profile-argument-r2,

device-minimum-Y-array-length = profile-argument-r3,

device-control-object = {SA,UA}

},

{

device-name = DVB, *("input" device object)*

device-default-CO-access = opposite of profile-argument-r1,

device-default-CO-initial-value = 1."true",

device-display-object = DOB,

device-minimum-X-array-length = profile-argument-r2,

device-control-object = profile-argument-r9,

device-control-object = {ST,UT},

device-control-object = TE

}

},

type-of-delivery-control = "simple-delivery-control".

8.6.4 Profile argument definitions

r1 - is mandatory and enables negotiation of which VT-user has update access to display object DOA.

It takes values "WACI", "WACA". It implies the asymmetric roles of the VT-users as "Application

VT-user" and "Terminal VT-user". If the value for DOA is "WACI", then the association initiator

is the "Application VT-user"; if the value of DOA is "WACA", then the association initiator is the

"Terminal VT-user". This profile argument is also used to determine which VT-user has access

to other VT objects as described above. Reference in the profile definition to "opposite of profile-

argument-r1" means that the alternative of the two possible values for profile- argument-r1 is to be

used. This argument is identified by the identifier for DO-access for display object DOA.

r2 - is optional and enables negotiation of a value for the VTE-parameter x-bound for the display

objects DOA and DOB. It takes an integer value greater than zero. This argument is identified

by the identifier for x-bound for display object DOA. Default is 80.

r3 - is optional and enables the negotiation of a value for the VTE-parameter

device-minimum-Y-array-length for device object DVA. It takes an integer value greater than zero;

if absent, a device of any length will be satisfactory.

NOTE - Indicates screen length.

r4 - is optional and provides for the negotiation of value(s) for the VTE-parameter

repertoire-assignment. The value of repertoire-capability is implied by the number of occurrences

of this argument. Default is specified by 9040.

r5 - is optional and provides for the negotiation of a value for the VTE-parameter DO-emphasis. The

default value is that given in ISO 9040, B.17.3. Refer to ISO 9040 B.17.4 for rules governing the

selection of non-default values.

r6 - is optional and provides for the negotiation of value(s) for VTE-parameters

foreground-colour-capability and background-colour-capability. Default is 8.

r7 - is optional and provides for the negotiation of a value for VTE-parameter

foreground-colour-assignment. Default is {"white", "black", "red", "cyan", "blue", "yellow", "green",

"magenta"}.

r8 - is optional and provides for the negotiation of a value for VTE-parameter

background-colour-assignment. Default is {"black", "white", "cyan", "red", "yellow", "blue",

"magenta","green"}.

r9 - is optional and enables negotiation of a termination control object. The value for this argument

is the value of CO-name for the termination control object, i.e. "TE"; if absent, no termination

control is defined.

r10 - is optional and provides for the negotiation of a value for the VTE-parameter y-window of the

DOA Display Object. Default is 24.

8.6.5 Profile dependent CO information

This profile makes use of five OIW registered Control Objects, SA, UA, ST, UT and TCCO. The CO-

access in each CO is defined within this profile.

8.6.6 Profile notes

8.6.6.1 Definitive notes

Only the first boolean of the default control object contained in each device object is defined. This boolean

is defined as the "on/off" switch for the device where the value "true" ="on" and "false" = "off". These

values were chosen so the initial value of the boolean, "true", means the device is initially "on" and data

to/from the display objects is being mapped to the device.

Only one boolean is defined in the standard echo control object, E. The semantics of this boolean is

defined such that "false" means "local echo off" and "true" means "local echo on"; these values were

chosen so echoing is initially "off" (which would provide security when a password is entered at the start

of a terminal session).

8.6.6.2 Informative notes

This profile models a scrolling device which is capable of scrolling both forwards and backwards. The

display pointer may be moved backwards to modify earlier lines. A typical use for this profile is for

applications where type-ahead may be advantageous and control over local echo "on"/"off" is required, e.g.

the type of application where a conventional teletypewriter device or ‘teletype-compatible’ video device

having ‘full duplex’ capability is often used. Display object DOA referred to above is typically mapped to

the display or printing device and display object DOB is typically mapped to the keyboard.

Use of A-mode enables "typed-ahead"into display object DOB, and such updates can be delivered

immediately to the peer VT-user, potentially reducing transmission delays. Such delivery will be forced,

and marked, by a termination condition or a VT-DELIVER. Type-ahead is at the discretion of the terminal

user.

Display object DOB has an unbounded y-dimension so as to provide a blank line for each new line entered.

Line-at-a-time forward scrolling is mapped onto an update-window (value zero) which allows NO backward

updates to preceding lines (x-arrays). The device-minimum-Y-array-length negotiated by

profile-argument-r3 can be used to indicate the number of lines (x-arrays) which should remain visible to

the human terminal user although specifically NOT available for update.

The ability to switch local echo "on" or "off" is always present; the ECHO control object is used for this

purpose.

8.6.7 Specific conformance requirements

None.

8.7 S-mode Paged Application profile

See Stable Agreements.

Annex A (normative) Specific ASE requirements SeeStableAgreements.

PART 14 - VIRTUAL TERMINAL September 1993 (Working)

Annex B (normative) Clarifications SeeStableAgreements.

PART 14 - VIRTUAL TERMINAL September 1993 (Working)

Annex C (normative) Object identifiers See Stable Agreements for Object Identifiers assigned to objects in the Stable Agreements. Object Identifiersbelowhavebeenassignedtoobjectsforwhichworkisstillinprogress. GeneralIdentifiers:

oiw-vt-rep OBJECT IDENTIFIER ::= { oiw-vt repertoire(2) } oiw-vt-font OBJECT IDENTIFIER ::= { oiw-vt font(3) } oiw-vt-colour OBJECT IDENTIFIER ::= { oiw-vt colour(4) } oiw-vt-directory OBJECT IDENTIFIER ::= { oiw-vt useOfDirectory(5) } Profiles defined by OIW VT SIG:

oiw-vt-pr-scroll-1989 OBJECT IDENTIFIER ::= { oiw-vt-pr scroll-1989(3) } Control Objects defined by OIW VT SIG:

oiw-vt-co-tcco-tc OBJECT IDENTIFIER ::= { oiw-vt-co-tcco tc(0) }

AnnexD (informative)

Recommendedpractice_OperatingXWindowSystemoverOSIupper layers

Thisannexprovidesa"recommendedpractice"fortheoperationoftheXWindowSystem(X)overanOSI upperlayerstack.The"recommendedpractice"providesaninterim

1solutionforanareanotaddressed bybasestandardsorexistingprofiles.ThisrecommendedpracticereflectsOIWagreement.

ItisrecommendedthatthisinterimsolutionbeusedwhenmappingXoveranOSIupperlayerstack. However,implementorsshouldnotethefollowing_futurespecificationsoftheregionalworkshopsmay possiblyresultindifferentsolutionsthanthoseproposedinthisrecommendedpractice.

D.1 Background

Xisagraphicaluserinterfacestandardwhichenablesausertoviewandgainaccesstomultiplecomputer applicationsfromasinglewindowormultiplewindowsonadisplayscreen.Xisbasedonaclient/server architecturewhichallowsapplicationsandresourcestobedistributedacrossanetwork.

TheXserverisasoftwareprogramthatisresidentonauser’sdisplayunitthatactsasanintermediary

betweentheuserandapplicationsrunningonalocalorremotesystem.TheXserveralsomaintains complexdatastructuressuchasspecificwindows,cursorsandfontswhichcanbereferencedandutilized byapplications.Inputfromthekeyboardand/ormouseiscollectedbytheX-serverandpassedtolocal and/orremoteapplicationsforprocessing.

ApplicationsarereferredtoasXclients.Theseapplicationsaccessthedisplayunitbysendingmessages totheXserverwhichisthenabletoperformtwodimensionaldrawingoflines,shapesandtext.

Xproductsarebasedonadefactostandard(MIT-X)maintainedbytheMITXConsortium.However,this specificationdoesnotprovidefortheoperationofXoverOSI-basednetworks.

TwoOSImappingspecificationswerecreatedtodefinetheoperationofXoveranOSIupperlayerstack: EWOSTechnicalGuide13(ETG13)andpart4ofANSIdpANSX.196(X3.196).Parts1-3wereintended todefinetheXprotocol.Part4wasbasedonETG13..X3.196neverprogressedbeyondthedraftproposal stage.ETG13wasapprovedbyEWOSin05/91.

ETG13explicitlydefines:

a) therequiredOSIupperlayerfacilities;

b) themappingoftheOSIupperlayerservicesforsendingandreceivingXprotocol.

Sincethecreationofthesedocuments,theISOISP11188-3CommonUpperLayerRequirements_Part 3:MinimalOSIupperlayerrequirements(CULR-3)cameintoexistence.CULR-3definestheminimalset

1ItisintendedthatthisRecommendedPracticewillbeprogressedasanRWStechnicalreport. 18

Annex E

— (normative)—

(ANNEX E WAS FORMALLY ANNEX D. THE WORKSHOP STYLES CHANGETHENUMBERINGAUTOMATICALLY.) OIWX— —

OSI— contributions — The following sections describe contributions by the OIW VT SIG to further X — — OSI—. Contributions in this — sectionarenotmeanttoreplaceanyexistingstandards,butaremeanttofillgapswherestandardsmay —notexist,orwheretheyarestillunderdevelopment. Wheneverpossible,contributionsinthissectionwill —bekepttechnicallyalignedwithanydevelopingstandards. — E.1 XDMCP

— —OSI—

E.1.1 Introduction — This section describes a means by which the protocol commonly known as XDMCP (X Display Manager —Control Protocol) may be mapped over the OSI Upper Layers. This specification is meant to provide one —solution to the problem of establishing an X connection in a pure-OSI environment. — Ingeneral,themappingofXDMCPtoOSIreliesonmuchoftheinformationalreadypresentintheX — — OSI—Part^— IV document, and as such, that information will not be duplicated here. — E.1.2 Functional overview — XDMCP provides for three different types of query operations: Query, IndirectQuery and BroadcastQuery. —The nature of the BroadcastQuery operation is such that is requires a connection-less environment, and —so will not be considered here. — In addition to the three query types, XDMCP provides for a number of other operations: ForwardQuery, —Willing, Unwilling, Request, Accept, Decline, Manage, Refuse, and Failed. The actual semantics of these —operations will not be discussed here except with regard to how they map to various OSI services. —Additional information on XDMCP operations may be found in the XDMCP protocol specification provided —by the MIT X Consortium. — E.1.2.1ACSE requirements — The ACSE requirements for XDMCP — — OSI—are the same as specified by X — — OSI—Part IV, with the exception of the — abstract and transfer syntaxes. — E.1.2.2Presentation requirements — XDMCP — —OSI—has the same presentation requirements as specified by X — — OSI—Part IV. —

E.1.2.3 Session requirements —

XDMCP — —

OSI— has the same session requirements as specified by X — —

OSI—

Part IV. —

E.1.2.4 Abstract and transfer syntaxes —

Note: We basically have two possible options here: one is to utilize the existing X — —

OSI— object identifiers as —

currently defined by EWOS, and request that EWOS register an abstract syntax which defines XDMCP, —

which would resemble: XDMCP-abstract-syntax :: = OBJECT IDENTIFIER { xosi, abstract-syntax(4) }. The —

other option would be to define the application context and abstract syntax under OIW, leaving the transfer —

syntax as specified by EWOS. —

E.1.2.5 XDMCP to OSI mapping —

The following sections outline how various XDMCP protocol elements are mapped to specific OSI services. —

The mapping is divided into four broad catagories, each describing mapping for specific operations based —

on the type of query. —

Note: that the following discussion includes a possible way to map the IndirectQuery function to OSI, —

however, with X.500 IndirectQuery may become an unneccessary feature. —

E.1.2.5.1 Query - display to manager —

An implementation claiming to support XDMCP — —

OSI— must support this minumum functionality. The Query —

functionality allows a display to query a specific manager for willingness to provide management services. —

A display may initiate an association with either the Query or IndirectQuery operation. Once the association —

is established, a display may request additional Query or IndirectQuery operations via P-Data regardless —

of the operation in the initial association request. —

Table 1 - XDMCP mapping for query/display to manager —

A-Associate Request & Indication

— Query—

A-Associate Response & Confirm

— Willing, Unwilling—

A-Release Request & Indication (manager initiates)

— <null>, Unwilling, Decline, Failed—

A-Release Response & Confirm —

P-Data (Display)

— Query, IndirectQuery, Request, Manage—

P-Data (Manager)

— Willing, Unwilling, Accept, Decline, Refuse, Failed—

E.1.2.5.2IndirectQuery - display to manager — A display or manager may optionally support IndirectQuery in addition to Query. Managers which receive —IndirectQuery requests in the A-Associate request which do not support IndirectQuery should refuse the

—association. — The manager which receives the IndirectQuery is known as the primary manager. The primary manager —will forward the IndirectQuery to secondary managers via a ForwardQuery operation. Optionally, the —primary manager may also indicate a willingness to perform the display management. As with secondary —managers which indicate a willingness to manage, the display is under no obligation to accept the primary

—managers offer, and may simply release the association. The primary manager may also choose not to

—send a Willing, in which case it may simply release the association. However, it may be desirable for the

—primary manager and/or the display to maintain the association for a period of time, so as to potentially be

—available for additional requests from the display. — Table 2 - XDMCP mapping for indirectquery/display to manager —

A-Associate Request & Indication

— IndirectQuery—

A-Associate Response & Confirm

— <null>, Willing—

A-Release Request & Indication (manager initiates)

— <null>, Unwilling, Decline, Failed — A-Release Response & Confirm — P-Data (Display)

— Query, IndirectQuery, Request, Manager — P-Data (Manager)

— Willing, Unwilling, Accept, Decline, Refuse, Failed — E.1.2.5.3IndirectQuery - manager to manager — This section specifies the mapping specifically for a primary manager to communicate a ForwardQuery —request to a secondary manager. — The IndirectQuery is sent by the display to a well-known manager (or primary manager), which in turn —forwards the request to a larger collection of secondary managers using ForwardQuery packets. — If associations haven’t been previously established between the primary manager and the secondary

—manager, an A-Associate will be sent with the ForwardQuery operation. If an association already exists,

—the primary manager will simply send the ForwardQuery operation via a P-DATA. It is up to the —implementation to determine how long an association between a primary and secondary manager should —be maintained as various tradeoff’s between association establishment overhead and maintaining an idle —association exist and have not been examined in this guide. — Either the primary manager or a number of secondary managers may respond to the query by by sending —a Willing response to the display which initiated the request. Secondary managers which are willing will —notify the requesting display by establishing an association with the display with the WIlling operation in —the A-Associate. — 27

PART 14 - VIRTUAL TERMINAL September 1993 (Working)

Table 3 - XDMCP mapping for indirectquery/manager to manager — A-Associate Request & Indication

— ForwardQuery — A-Associate Response & Confirm — P-Data

— ForwardQuery — E.1.2.5.4Indirect query - manager to display — Thissectionspecifiesthemappingforasecondary managerwhichhasreceivedaForwardQueryrequest, —and wishes to respond with a WIlling to the requesting display. To perform this function, the secondary —manager must first establish an association with the Willing operation in the A-Associate request. The

—display may accept the A-associate yet not immediately respond to the Willing indication. If the display

—subsequently decides not to accept the Willing from the manager in question, it will simply release the —association. — Table 4 - XDMCP mapping for indirectquery/manager to display — A-AssociateRequest&Indication

— Willing— A-AssociateResponse&Confirm

— <null>,Request — A-ReleaseRequest&Indication(managerinitiates)

— <null>,Failed — A-ReleaseRequest&Indication(displayinitiates) — P-Data(manager)

— Accept,Decline,Refuse — P-Data(display)

— Request,Manage —